DC520N - DW979 - GSA64 Cordless V.S.R. Screwdriver

Item 1, clamshell pair: The date code is located on the bottom of the handle.

Item 7, switch: Static protection must be used when handling the switch.

Item 12, locator: Tighten to 16.0 - 18.0 Nm .

Item 18, screw: Tighten to 1.5 - 2.0 Nm .

Item 36, seal: The dust seal must not be pinched between the clamshells.

Lubrication:

Lubricate clutches and spindles with approx 0.5 gms of grease.

Maintenance checks

i) refer to standard maintenance routine.