R10027
EPT1151/3.

Instructions.
The chain for raising and lowering the table should be tensioned to 9 - 14 mm of movement (32).

Use 17 mm spanner to remove the feed control mechanism (223).

Use 3 mm key to remove the cutterblock drive pulley (247).

There is 3 - 5 mm of end play on the winding handle pinion (23).

Item 402, guard sa, includes items 401, 417.