NOTES:
  1		Date Code located on housing at battery insert area.
  9		Grease must coat lug faces, bearing journals, cam path and gear teeth. See below.
18		Torque to 15 ± 2 in-lbs (1.7 ± 0.2 Nm)
21		Torque to 20 ± 2 in-lbs (2.3 ± 0.3 Nm)

LUBRICATION
1. DISTRIBUTE TOTAL OF 3.8 – 10.6 GRAMS OF G2008 GREASE (34138513-05) IN     
    LOCATIONS NOTED IN THIS DOCUMENT.  (Pictures for reference only)

2. DISPENSE G2008 GREASE AND APPLY TO PARTS AS SHOWN IN PICTURES.

See Note 2
2.0 +/- 1.0 Grams
Both Cam Grooves

See Note 2
1.1 +/- 0.7 Grams

See Note 2
1.1 +/- 0.7 Grams

                          

See Note 2
1.0 +/- 0.5 Grams

See Note 2
1.5 +/- 0.5 Grams

See Note 2
0.5 Max Grams

Use proper dispensing method to apply Nyogel NYE grease to the POWER TERMINALS of the terminal block 8 places as shown.  (0.02 +/- 0.005 grams total). PICTURES ARE FOR REFERENCE ONLY.

GREASE POWER TERMINALS ONLY

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

When servicing Double Insulated Tools, it is extremely important that ONLY IDENTICAL REPLACEMENT PARTS BE USED and that REASSEMBLY OF TOOL IS IDENTICAL TO THE ORIGINAL ASSEMBLY.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.